Table below covers main Wellington City Council scheduled roadworks for August 2025.

| **LOCATION** | **TYPE OF WORK** | **INDICATIVE DATES** | **TRAFFIC MANAGEMENT**  **(unless noted, all work is day work)** | **OTHER INFORMATION** |
| --- | --- | --- | --- | --- |
|  |  | **CBD** |  |  |
| **Various** | Reactive | 01 August to 31 August | Stop/go |  |
| **Various** | Roadmarking | 01 August to 31 August | Stop/go |  |
|  |  | **Northen Suburbs** |  |  |
| Sunshine Ave, **Karori** | Kerb, channel and footpath | 11 August to 27 August | Stop/go |  |
| Victory Ave, **Karori** | Footpath maintenance and road repairs | 28 August to 04 September | Stop/go |  |
| Homewood Ave, **Karori** | Footpath maintenance and digouts | 12 August and 28 August | Stop/go |  |
| Newcombe Cres, **Karori** | Footpath maintenance and road repairs | 11 August to 18 August | Stop/go |  |
| Old Karori Rd, **Karori** | Kerb and channel | 19 August to 23 August | Stop/go |  |
| Seaforth Tce, **Karori** | Kerb, channel and footpath maintenance | 25 August and 16 September | Stop/go |  |
| Blakey Ave, **Karori** | Kerb, channel and footpath maintenance | 21 July to 01 August | Stop/go |  |
| Birdwood St, **Karori** | Remedial works to failed slope | 01 August to 31 August | One lane closure with traffic lights |  |
| Makara Road, **Karori** | Retaining wall renewal | 01 August to 31 August | Downhill lane Closure |  |
| Allington Street culvert, **Karori** | Bridge Upgrades | 01 August to 31 August | One lane closure |  |
| Helston Rd, **Johnsonville** | Footpath maintenance and digouts | 05 August to 11 August | Stop/go |  |
| Ironside Rd, **Johnsonville** | Kerb, channel and footpath maintenance | 30 July to 08 August | Stop/go |  |
| Stewart Derive, **Johnsonville** | Retaining wall renewal | 1 August to 31 August | Footpath closure |  |
| Beauchamp St, **Tawa** | Kerb, channel and footpath maintenance | 04 August to 06 September | Stop/go |  |
| Leadley Lane, **Tawa** | Water cutting | 01 August | Stop/go |  |
| Taylor Tce, **Tawa** | Water cutting | 01 August | Stop/go |  |
| Findlay St, **Tawa** | Water cutting | 04 August | Stop/go |  |
| Tawa Main Road, **Tawa** | Pedestrian crossing | 01 August to 31 August | Stop/Go | Installation of pedestrian crossing lighting |
| Hutt Rd-South, **Ngaio** | Water cutting | 04 August | Stop/go |  |
| Khandallah Road – Cockayne Road, **Ngaio** | Road Marking | 01 August to 31 August | Stop/Go | Cycleway shoulder marking |
| Whakowhai Street, **Ngaio** | Road Marking | 01 August to 31 August | Stop/Go | Cycleway shoulder marking |
| Ravi St, **Khandallah** | Footpath maintenance | 24 July to 04 August | Stop/go |  |
| Box Hill, **Khandallah** | Street light installation | 01 August to 31 August | Stop/Go | Bollard installation |
| Khandallah Road to Simla Cres,  **Khandallah** | Parking Bay Construction | 01 August to 31 August | Stop/Go | Parking layby construction |
| Grovenor Terrace Wall, **Wadestown** | Emergency Rout Wall Upgrades | 01 August to 31 August | One Lane closure |  |
| Randwick Rd, **Northland** | Dish channel | 25 July to 09 August | Stop/go |  |
|  |  | **SOUTHERN** |  |  |
| **Various** | Reactive | 01 August to 31 August | Stop/go |  |
| Evans Bay Parade, **Hataitai Beach** | Cycleway Construction | 01 August to 31 August | Stop/Go | Renewal of Sea Wall |
| Evans Bay Parade, **Hataitai Beach** | Cycleway Construction | 01 August to 31 August | Stop/Go | Construction of cycleway |
| Evans Bay Parade, **Hataitai Beach**  (Niwa to dog Park) | Cycleway Construction | 01 August to 31 August | Stop/Go | Construction of cycleway |
| Ohiro Road, **Brooklyn** | Parking Bay Construction | 1 August to 31 August | Stop/Go | Construction of parking bay and line marking |
| Mortimer Terrace, **Aro Valley** | Retaining Wall | 1 August to 31 August | Road closure, pedestrian and resident access maintained |  |

**Definitions:**

*Dig out* – *a repair to a small section of the road structure*

*Pre-seal repairs* – *structural repairs to small sections of the road. We usually combine this with repairing or replacing sections of the pedestrian footpath, kerb and channel. This work is done two to three months before the surfacing work. This gives the road repairs time to settle and cure.*

Sump *– road drain*

*Water Cutting - Water blasting to remove the top surface of a road – noisy work*

*TTM – temporary Traffic Management*

*TSL – Temporary Speed Limit*